Erasing the flash (removes software and database from the panel)
1. Power off panel.
2. Hold down 'F4' 'esc' & 'Enter'.
3. with the keys still held, power on.
4. The panel should now be in boot transfer mode.